Udp client

#include <stdio.h>

#include <stdlib.h>

#include <unistd.h>

#include <string.h>

#include <sys/types.h>

#include <sys/socket.h>

#include <arpa/inet.h>

#include <netinet/in.h>

#define PORT 8080

#define MAXLINE 1024

// Driver code

int main() {

int sockfd;

char buffer[MAXLINE];

char \*hello = "Hello from client";

struct sockaddr\_in servaddr;

// Creating socket file descriptor

if ( (sockfd = socket(AF\_INET, SOCK\_DGRAM, 0)) < 0 ) {

perror("socket creation failed");

exit(EXIT\_FAILURE);

}

memset(&servaddr, 0, sizeof(servaddr));

// Filling server information

servaddr.sin\_family = AF\_INET;

servaddr.sin\_port = htons(PORT);

servaddr.sin\_addr.s\_addr = INADDR\_ANY;

int n, len;

while (1) {

bzero(buffer, MAXLINE);

printf("\tClient: ");

n = 0;

while ((buffer[n++] = getchar()) != '\n');

sendto(sockfd, (const char \*)buffer, strlen(hello),

MSG\_CONFIRM, (const struct sockaddr \*) &servaddr,

sizeof(servaddr));

printf("message sent.\n");

n = recvfrom(sockfd, (char \*)buffer, MAXLINE,

MSG\_WAITALL, (struct sockaddr \*) &servaddr,

&len);

buffer[n] = '\0';

printf("\tServer : %s", buffer);

if (strncmp(buffer, "exit", 4) == 0) {

break;

}

}

close(sockfd);

return 0;

}